# Rack Database Structure: Runs table

Structural fields
idx | integer | Unique index number for each run, automatically assigned
name | string | Descriptive name for this scenario
Deprecated fields
comment | string | These fields have all been replaced with new ways of doing things.
constraints | integer |
oldcons | integer |
newsams | integer |
Run parameter fields
min | integer | minimum number of racks/facilities to select
max | integer | maximum number of racks/facilities to select
numcombos | integer | number of combinations at each number of racks/facilities, usually 1000
tblname | string | name of the table to store the output data in
outputdb | string | name of the database tblname is in
outputpath | string | where to put the charts for this run inside the PLUM output directory.
topology | string | name of the rack topology to use, links to name in topology table
ignorezeros | boolean | if this is true, then resources with a zero capability never exceed no matter what the total usage is.
Resource fields
MLE | number |
stowage | number |
upmass | number |
bulk | number |
rack_overhead | number |
crewtrng | number |
crewtime | number |
power | number |
keepalive | number |
Networking fields
avg_uplink | number |
avg_ethernet | number |
avg_1553 | number |
avg_HRL | number |
avg_downlink | number |
peak_uplink | number |
peak_ethernet | number |
peak_1553 | number |
peak_HRL | number |
peak_downlink | number |
peak_uplink_duration | number |
peak_downlink_duration | number |
peak_1553_duration | number |
peak_ethernet_duration | number |
peak_HRL_duration | number |
video_uplink | number |
video_downlink | number |
video_rate | number |
Constant fields
inclength | number | the number of days in an increment. Usually 90 or 180.
middeckmass | number |
passiveMLE | number |
passive_middeck_mass | number |
sams_power | number | The power usage of SAMS. Added to the power requirement of the rack containing SAMS.
hskpg | number |
ku_power | number |
pl_power | number |
stowage_MLEs | number |
Cold stowage fields
cs_p4_asc | number |
cs_p4_orb | number |
cs_p4_desc | number |
cs_m20_asc | number |
cs_m20_orb | number |
cs_m20_desc | number |
cs_m80_asc | number |
cs_m80_orb | number |
cs_m80_desc | number |
cs_m180_asc | number |
cs_m180_orb | number |
cs_m180_desc | number |